REQ-001: The system shall allow users to log in using multi-factor authentication.

REQ-002: All user data must be encrypted at rest and in transit.

REQ-003: The software shall process sensor inputs within 100 milliseconds.

REQ-004: The system should display an error message if network connection is lost.

REQ-005: The application shall support both dark mode and light mode.